

**Pelican 100 Watt Siren**

**Operating Manual and Installation Instructions**

A close up of electronics

Description automatically generated

**Hawk Warning Stick and Arrow Stick Control Box**

## Operating Manual and Installation Instructions

**Warnings and Notices for Users and Installers**

**WARNING: Take CAUTION when installing**

This document must be delivered to and read by the end user and installer as it serves to provide you with the required information for proper and safe use of your LEDEQUIPPED product. Before operating this or any LEDEQUIPPED products the user and installer must read this manual all the way through. You will find important information in this manual that could prevent property damage and/or serious injury to the user and installer. LEDEQUIPPED products are intended to alert pedestrians and other operators of the presence of personnel, the operation of emergency vehicles, an emergency site, and any warning needs. It is your responsibility to make sure you can proceed safely before driving against traffic, entering an intersection, responding to a high rate of speed, or walking on or around traffic lanes.

Your LEDEQUIPPED emergency vehicle devices should be tested daily to insure the device and all it's functions are operating correctly. If you experience a malfunction contact LEDEQUIPPED's Customer Service immediately for troubleshooting options, or a warranty or service claim. You must ensure sure that the projection of the visual and audible is not blocked by vehicle components (i.e.: open trunks, visors, compartment doors), vehicles, other obstructions, or people. LEDEQUIPPED's sirens and other audible devices project sound in a forward direction and should be installed in a forward direction that faces away from the occupants of the vehicle.

This is professional grade equipment and is intended for strict use by authorized personal only. It is the user's responsibility to understand and obey all laws regarding emergency warning devices. You must know and be familiar with all applicable city, sate, and federal laws and regulations prior to the use of emergency vehicle warning devices. LEDEQUIPPED assumes no liability for any loss resulting from the use of this warning device. Proper installation is vital to the performance of the warning devices and safe operation of the emergency vehicle. Since the operator is under stressful environments the equipment must be properly wired and mounted to ensure effectiveness and safety. Therefore, controllers must be properly installed and placed within convenient reach of the operator so eye contact with the roadway is never lost. The effectiveness of your LEDEQUIPPED equipment is highly dependent upon correct mounting and wiring.

Improper wiring and mounting of the warning device will reduce the output and performance of the equipment. Emergency warning devices frequently require high electrical voltages and/or currents. Properly protect and use caution around live electrical connections. Grounding or shorting of electrical connections can cause high current arcing, which can cause severe personal injury and/or serious vehicle damage, including fire. Electromagnetic interference can be caused by many electronic devices used in emergency vehicles. To ensure that this doesn't happen to you, lights bars should be mounted a minimum of 12" - 34" from the radio antenna and do not power your equipment from the same circuit or share the same grounding circuit with radio communication equipment. After installation test all the vehicles equipment together to ensure everything operates free of interference. Driver and/or passenger airbags bags (SRS) will impact the way you mount your equipment. Any equipment installed in the deployment area of the airbags will damage or dislodge the airbags and sensors. This will also reduce the effectiveness of the airbags to protect the passengers and therefore these areas must be avoided. Installers must make sure that this equipment along with any parts, hardware, wiring, power supplies, and switch boxes do not interfere with the airbags, SRS wiring, or sensors. All LEDEQUIPPED equipment needs to be mounted and installed according to the vehicle manufactures instructions and securely attached to a part of the vehicle of sufficient strength to withstand the forces applied to the equipment. This device should be permanently mounted within the zones specified by the vehicle manufactures. This especially applies to equipment mounted on the exterior of the vehicle to avoid dislodging. When mounting units on the interior of the vehicle by a method other than permanent mount is discouraged as the it may become to detached under aggressive driving conditions such as sudden breaking, collision, or swerving.

## Important Points for Your Safety and Longevity of your Equipment

Installers are required to have a good understanding of automotive electronic, systems and procedures for proper installation.

* One should not stare directly into the LEDs as momentary blindness and/or eye damage may occur.
* One should not take any lights through a car wash. Use only water to clean the outer body/lens of your equipment. –
* One should not use a pressure washer to clean any LEDEQUIPPED products. Inspect and test your product daily to insure it operates properly and is mounted correctly.
* One should not cut wires or work on a unit while the unit is still connected to a power source.
* One should not install this product or rout any wires through or in the deployment area of the airbag. Doing so may cause serious personal injury as it will damage or reduce the effectiveness of the airbag by causing the unit to become a projectile.

Reference the owner's manual for your vehicle to find the airbag deployment area. The User/Installer assumes all responsibility to determine proper mounting location, based on providing ultimate safety to all passengers in the vehicle.

* If the product requires you to drill holes the installer must ensure that the drilling process does not damage any vehicle components or other vital parts. Check all sides of the mounting surface before beginning to drill. Make sure to deburr all drilled holes and remove any metal remnants or shards to avoid injury and wires from becoming spliced. Grommets are to be installed in all wire passage holes.
* For LEDEQUIPPED products to operate at optimum efficiency a secure and good electrical connection to the Batteries Ground Post must be made. The recommended procedure requires the unit's ground wire be connected directly to the NEGATIVE (-) battery post.

**Accessories**

The following parts are included with the Pelican 100w Siren.

A close up of electronics

Description automatically generated A picture containing electronics, indoor, sky, black

Description automatically generated

|  |  |  |
| --- | --- | --- |
| Pelican 100w Siren Amplifier |  | Handheld Siren and Accessory Control Unit |

A close up of a red cable

Description automatically generated A close up of a cable

Description automatically generated

|  |  |  |
| --- | --- | --- |
| Four (4) Pin 12v Power Wiring Harness |  | Eleven (11) Pin Siren and Accessory Control Wiring Harness |

A close up of a black device

Description automatically generated

RJ45 Handheld Controller Extension Cable

## Instructions for Wiring and Operation

Installation and Wiring

To ensure proper installation installers are required to have a good understanding of automotive electronic, systems and procedures for proper installation.

When you are drilling into the vehicle's surfaces, ensure that the area is free of any electrical wires, vehicle upholstery, fuel lines, etc. that could be damaged. All wiring passing through drilled holes should use grommets and silicone sealant to prevent wire or moisture damage when passing through compartment walls.

WARNING! Larger wires and secure or tight connections will ensure longer service life for your product. It is highly recommended that soldered connections have heat shrink used to protect the connection. Special attention should be given to the location and method of splicing wires to make electrical connections to protect these splices from lost power or connection and corrosion.

Insulation displacement connectors are not to be used. To reduce voltage drop, minimize the number of splices in the wires. The current carrying capacity of wires and fuses will be significantly reduced under high ambient temperature (e.g. under the hood).

All wires should be in accordance with the minimum wire size and other recommendations made by the manufacturer and be protected from hot surfaces and moving parts. Grommets, cable ties, looms, and other installation hardware should be used to anchor and protect all wiring. Fuses should be properly sized and located as close to the power take off points as possible to protect the wiring and device. To protect against short circuits, a fuse is included by LEDEQUIPPED for all products. Do NOT use a fuse with a higher amp rating than the initial fuse included.

# 

# Fig. 1

# A circuit board Description automatically generated

# The Pelican 100w Siren is designed for easy connection to your vehicle and comes with prewired 12v+ and 12v- power wires. All wiring for the Pelican 100w Siren is connected using the provided eleven (11)-pin and four (4)-pin wiring harnesses using screw down wire terminals for ease of installation. (Fig. 1). In addition to the provided wiring harnesses, the Pelican 100w Siren’s handheld control is connected using a preinstalled RJ-45 connector and controller input.

# Wiring the Pelican 100 Watt Siren

# Wiring the Pelican 100w Siren is made easy through the use of screw down wire terminals. Please note that the 12v + (Positive/Red Wires) and 12v – (Negative/Black Wires) wiring connections must be made to an appropriate 12v power source and ground, in order for your Pelican 100w Siren to function properly. The images included below provides a visual representation for how to wire the four (4) pin (Figure 3) and eleven (11) pin Pelican 100w Siren wiring harnesses (Figure 3).

# Fig. 2

# A picture containing text Description automatically generated

|  |  |
| --- | --- |
| Four (4) Pin Wire Harness | |
| Terminal | Function |
| Sirens DC 12v INPNT | 12v + (Positive) – For Siren Installation |
| Lights DC 12v INPNT | 12v + (Positive) – For Accessory Installation (Lights) |
| Black – | 12v – (Negative) |

# Fig. 3

# A circuit board Description automatically generated

|  |  |
| --- | --- |
| Eleven (11) Pin Wire Harness | |
| Terminal | Function |
| LTA (1) | 12v + (Positive) Output – For Accessory (Light) L1 |
| LTB (2) | 12v + (Positive) Output – For Accessory (Light) L2 |
| LTC (3) | 12v + (Positive) Output – For Accessory (Light) L3 |
| LTD (4) | 12v + (Positive) Output – For Accessory (Light) L4 |
| LTE (5) | 12v + (Positive) Output – For Accessory (Light) L5 |
| LTF (6) | 12v + (Positive) Output – For Accessory (Light) L6 |
| VCC (+) | Switched Power - Must be connected to a 12v + (Positive) Source |
| VDC (↓)\* | Vehicle Horn Relay – 12v + (Positive) Output |
| VDC (↑)\* | Vehicle Horn |
| R + | 100W Speaker Positive (+) |
| R – | 100W Speaker Negative (-) |

# \*In order to utilize the vehicle horn button to switch siren tones, you must cut the wire that connects the Vehicle Horn Relay (12v +) to the Vehicle Horn and connect the VDC (↓) wire to the wiring coming from the horn relay and the VDC (↑) wire to the wire coming from the horn.

# Pelican 100 Watt Siren Wiring Diagram

# A circuit board Description automatically generated

# All wiring connections should be secured using appropriate automotive connectors or through the use of soldered connections. All connections should be protected by using heat shrink wire wrap in order to protect the connection. Special attention should be given to the location and method of splicing wires to make electrical connections to protect these splices from lost power or connection and corrosion.

**Connecting the Pelican 100w Siren Handheld Remote Control Unit**

The Pelican 100w Siren Handheld Remote Control Unit is designed to use a standard RJ45 connection to connect to the Pelican 100w Siren Amplifier. Simply plug the handheld remote control unit into the ‘Control’ port on the Pelican 100w Siren Amplifier to connect the unit. In addition, a RJ45 extension cable comes included with the Pelican 100w Siren. This extension cable can be used to extend the reach of your handheld remote control unit so that the Pelican 100w Siren Amplifier can be mounted anywhere within your vehicle. Plug in the RJ45 extension cable into the ‘Control’ port on the Pelican 100w Siren Amplifier and connect the handheld remote control unit into the RJ45 connection on the opposite end of the extension cable to expand the reach of our handheld remote control unit.

**Mounting the Pelican 100w Siren Amplifier Unit**

The Pelican 100w Siren is designed to be mounted directly into your preferred vehicle location. There are four (4) mounting holes on the Pelican 100w Siren amplifier unit, which should be used to secure the unit to your vehicle in your preferred vehicle location. Please ensure that before mounting or drilling holes in your vehicle to mount the unit, that the area for mounting is clear of any vehicle wiring components and that the unit is mounted in such a way that it will not interfere with any of your vehicle’s safety components, including Air Bags. As noted above, included with the Pelican 100w Siren is an RJ45 extension cable that can be used to extend the reach of your handheld remote control unit from the mounting location of the Pelican 100w Siren amplifier unit.

Operation

The Pelican 100w Siren includes a lighted handheld remote control unit to operate both the optional accessories/lights as well as the included siren and horn tones. There are six (6) six soft touch buttons to operate those accessories that you may choose to control using the Pelican 100w Siren (L1 – L6). In addition, there are eight (8) soft touch buttons to operate each of the included siren and horn tones that are included with your Pelican 100w Siren. The main ‘Power’ button allows for quickly and easily powering the entire unit on and off.

A picture containing electronics, indoor, sky, black

Description automatically generated

The respective button functions are:

**Power** Power on and power off of the Pelican 100w Siren and Accessories/Lights**.**

**L1 – L6** Individual control for up to six (6) discrete accessories/lights that can be controlled by the Pelican 100w Siren.

**Horn** Air Horn Tone

**Siren** Holding this button will allow the Wail siren tone to reach its peak and hold that tone until this button is released. This is a manual use function and does not engage a constant siren tone.

**Mech** Mechanical Siren Tone.

**Yelp** Yelp Siren Tone.

**Wail** Wail Siren Tone

**HiLo** High-Low Siren Tone.

**Tool** Tool Siren Tone.

**DHSR** Phaser Siren Tone.

The Pelican 100w Siren Handheld Remote Control Unit is equipped with an LED backlight which changes color to illuminate the current functions that are in use.

At LEDEQUIPPED, we know that you need affordable lighting for your police, EMS, fire, construction, or towing vehicles and that safety and reliability are important to you. That’s why all of our LED products feature powerful up do date Generation LED lighting, perfect for your police, fire, construction, or EMS vehicle. LEDEQUIPPED focuses on a mission to carry out business ethically and with integrity, provide powerful products of the highest quality, maintain excellent and affordable prices, and to establish an unparalleled customer service relationship beginning with establishing trust with our costumers. As a provider of emergency vehicle lighting, we value the honesty, professionalism, and expertise present within our customer base

For any questions regarding our products, contact us by calling us at +1 800-846-3940 or email us at sales@ledequipped.com.

